FIG Forth 6502 V1.7 for CPM-65 JC-][ Version

Implementation

Registers

X stack pointer

Y Pointer for IP in NEXT

N 8 bytes scratch

R/W

1. Block is SCR #3, start addres is LO (=$8000)
2. Highest available SCR is #19 (= $C800 - $CBFF)

Compiler Security Check

Load CS.BLK

Run CS – Search parameter is fixed to $FB as low byte in PFA

Must be run after every modification in the FIG-FORTH source